

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,320 | **69’** | **23’** | **9** | **17.85 Kips** | **25.0 Kips** |
| Engines: | **Face Wires:** | **Fresh Water:** | **Fuel Oil:** |
| Twin CumminsQSK19-M | **7/8”x110’** |  |  |
| Propellers: | **Tow Winch:** | **Bow Winch:** |
| Twin |  |  |
| Gross Tonnage: | **Call Sign:** | **Official Number:** |
| 108 | **WV8240** | **298912** |
| Note: |
| Tank Vessel Escort Certified |