

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Horsepower: | Length: | Beam: | Deep Draft: | Astern Bollard: | Ahead Bollard: |
| 1,320 | **69’** | **23’** | **9** | **17.85 Kips** | **25.0 Kips** |
| Engines: | **Face Wires:** | | | **Fresh Water:** | **Fuel Oil:** |
| Twin Cummins  QSK19-M | **7/8”x110’** | | |  |  |
| Propellers: | **Tow Winch:** | | | **Bow Winch:** | |
| Twin |  | | |  | |
| Gross Tonnage: | **Call Sign:** | | | **Official Number:** | |
| 108 | **WV8240** | | | **298912** | |
| Note: | | | | | |
| Tank Vessel Escort Certified | | | | | |